<?xml version="1.0"?>

<fmodel>
    <geofile>analytic_example_model</geofile>
    <geofile_debug>analytic_example_model_debug</geofile_debug>
    <subdomains>
        <subdomain name="innner_volume" material="inner_material" physid="100"/>
        <subdomain name="volume_shell" material="shell_material" physid="101"/>
        <subdomain name="bounding_box" material="outer_material" physid="102"/>
    </subdomains>
    <boundaries>
        <boundary name="left_boundary" physid="1"/>
        <boundary name="right_boundary" physid="2"/>    
    </boundaries>
    <materials>
        <material name="inner_material" conductivity="2.0" permittivity="120"/>
        <material name="shell_material" conductivity="0.1" permittivity="2e6"/>
        <material name="outer_material" conductivity="1.0" permittivity="80"/>
    </materials>
    <boundary_conditions>
        <boundary_condition name="left_plate" type="dirichlet" boundary="left_boundary" value="0.5"/>
        <boundary_condition name="right_plate" type="dirichlet" boundary="right_boundary" value="-0.5"/>
    </boundary_conditions>    
    <frequency value="3.5e4"/>   
</fmodel>